{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Inflitration Reduction","Tables"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Inflitration Reduction","index":0,"n_rows":29,"n_cols":14,"rows_kept":29,"cut":false,"hidden":false,"merged":[[12,1,12,2],[12,3,12,4],[12,5,12,12],[5,0,5,13],[8,0,8,13],[9,0,9,13],[11,0,11,4],[11,5,11,12],[0,0,0,13],[1,0,1,13],[3,0,3,3],[3,4,3,13],[4,0,4,13],[17,3,17,4],[15,1,15,2],[15,3,15,4],[15,5,15,12],[13,1,13,2],[13,3,13,4],[13,5,13,12],[14,1,14,2],[14,3,14,4],[14,5,14,12],[16,3,16,4],[16,5,16,12],[17,5,17,12],[16,1,16,2],[17,1,17,2],[18,1,18,2],[18,3,18,4],[20,0,20,13],[21,0,22,0],[25,0,26,0],[25,5,26,5],[21,13,22,13],[23,1,24,4],[23,5,24,5],[23,10,24,10],[23,13,24,13],[18,5,18,12],[21,11,22,12],[23,11,24,12],[23,0,24,0],[21,1,22,4],[27,13,28,13],[25,13,26,13],[27,10,28,10],[27,6,27,9],[28,6,28,9],[27,11,28,12],[25,6,26,9],[25,11,26,12],[21,5,22,5],[21,10,22,10],[27,5,28,5],[25,10,26,10],[27,0,28,0],[25,1,26,4],[27,1,28,4],[21,6,22,9],[23,6,23,9],[24,6,24,9]]}
["Dry Bulb Airside Economizer"]
["(Gas Cooling)"]
[]
["Description of UCRM:",null,null,null,"(Data needed:  use of space, schedule, inside temp during free cooling season, and"]
["inside relative humidity during free cooling season)"]
[]
[]
[]
[]
[]
[]
["Data needed for calculations",null,null,null,null,"Description",null,null,null,null,null,null,null,"Resource"]
["A)",null,null,"cfm",null,"Airflow of AHUs utilizing free cooling"]
["B)",null,null,"Btu/lb",null,"Enthalpy inside the facility (Use Table 17 or Psych. Chart)",null,null,null,null,null,null,null,"Table 17"]
["C)",null,null,"Btu/lb",null,"Enthalpy outside the facility",null,null,null,null,null,null,null,"Table 17"]
["D)",null,null,"hrs/yr",null,"Annual Free Cooling Hours",null,null,null,null,null,null,null,"Table 17"]
["E)",null,null,"COP",null,"Efficiency of Cooling System"]
["F)",null,null,"$/Mcf",null,"Natural Gas Rate"]
["G)",null,null,"$",null,"Cost of Project, Including Design"]
[]
["Calculations"]
["H)","Cooling Energy Savings",null,null,null,"=","4.5 * A * (B - C) * D",null,null,null,"=",{"$f":"4.5*B13*(B14-B15)*B16","v":0},null,"Btu/yr"]
[]
["I)","Annual Cooling Electrical Energy Savings",null,null,null,"=","H",null,null,null,"=",{"$f":"L22/(B17*1030000)","v":{"$error":"#DIV/0!"}},null,"Mcf/yr"]
[null,null,null,null,null,null,"E * 1,030,000 Btu/Mcf"]
["J)","Annual Cooling Cost Savings",null,null,null,"=","I * F",null,null,null,"=",{"$f":"L24*B18","v":{"$error":"#DIV/0!"}},null,"$/yr"]
[]
["K)","Simple Payback",null,null,null,"=","G",null,null,null,"=",{"$f":"B19/L26","v":{"$error":"#DIV/0!"}},null,"yrs"]
[null,null,null,null,null,null,"J"]

{"sheet":"Tables","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}