{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Timeclock Control","Tables"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Timeclock Control","index":0,"n_rows":26,"n_cols":14,"rows_kept":26,"cut":false,"hidden":false,"merged":[[5,0,5,13],[0,0,0,13],[1,0,1,13],[3,0,3,3],[3,4,3,13],[4,0,4,13],[6,0,6,13],[7,0,7,13],[9,0,9,4],[9,5,9,12],[10,1,10,2],[10,3,10,4],[10,5,10,12],[13,5,13,12],[11,1,11,2],[11,3,11,4],[11,5,11,12],[12,1,12,2],[12,3,12,4],[12,5,12,12],[13,3,13,4],[13,1,13,2],[16,1,16,2],[16,3,16,4],[16,5,16,12],[14,1,14,2],[14,3,14,4],[14,5,14,12],[15,1,15,2],[15,3,15,4],[15,5,15,12],[22,10,23,10],[25,6,25,9],[24,11,25,12],[24,13,25,13],[24,0,25,0],[24,1,25,4],[24,5,25,5],[24,10,25,10],[24,6,24,9],[22,11,23,12],[22,13,23,13],[22,0,23,0],[22,1,23,4],[22,6,23,9],[22,5,23,5],[18,0,18,13],[19,0,19,13],[20,0,21,0],[20,1,21,4],[20,11,21,12],[20,13,21,13],[20,5,21,5],[20,6,20,9],[20,10,21,10],[21,6,21,9]]}
["Timeclock Control of Motor Loads"]
["(Non Air-Conditioned Space)"]
[]
["Description of UCRM:"]
[]
[]
[]
[]
[]
["Data needed for calculations",null,null,null,null,"Description",null,null,null,null,null,null,null,"Resource"]
["A)",null,null,"hp",null,"Horsepower of Motor to be Controlled"]
["B)",null,null,"%",null,"Motor Efficiency (Nameplate or Table 9)",null,null,null,null,null,null,null,"Table 9"]
["C)",null,null,"%",null,"Motor Load Factor"]
["D)",null,null,"hrs/yr ",null,"Hours per Year that Motor will be shut off  =  hrs/day  *  days/yr   "]
["E)",null,null,"$/kWh",null,"Electrical Energy Rate - Summer"]
["F)",null,null,"$/kWh",null,"Electrical Energy Rate - Winter"]
["G)",null,null,"$",null,"Installed Cost per Timeclock"]
[]
["Calculations"]
["Electric Heating Alternative:"]
["H)","kWh Saved",null,null,null,"=","0.746 kW/hp * A * C * D",null,null,null,"=",{"$f":"(0.746*B11*(B13/100)*B14)/(B12/100)","v":{"$error":"#DIV/0!"}},null,"kWh/yr"]
[null,null,null,null,null,null,"B"]
["I)","Annual Cost Savings",null,null,null,"=","H * (E + F) / 2",null,null,null,"=",{"$f":"L21*(B15+B16)/2","v":{"$error":"#DIV/0!"}},null,"$/yr"]
[]
["J)","Simple Payback",null,null,null,"=","G",null,null,null,"=",{"$f":"B17/L23","v":{"$error":"#DIV/0!"}},null,"yrs"]
[null,null,null,null,null,null,"I"]

{"sheet":"Tables","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}